WILL-BURT LIGHT TOWER SPECIFICATIONS
Night Scan Chief NS 2.3-3000-2 FRC Optimum 240 VAC
Model Number 720748041

A Will-Burt Night Scan Chief Series light tower shall be provided.   The horizontal surface mounted tower shall be raised electrically and pneumatically.

Mounting provisions shall be provided with the assembly.   The installation of unit shall be as follows:
1.  Light tower installation location: 
2.  Floodlight and tower control location:

Design and Construction

The tower shall be a series of graduated extruded aluminum tubes that nest one inside another.  The tower shall have an extended height of approximately 7.5 ft. / 2.3 m above the mounting location and a stowed height of approximately 9.375" / 23.8 cm above the mounting surface.  The tower shall be approximately 40.375” / 102.6 cm wide by 51.25” / 130.2 cm in length.  The tower shall be designed to sustain the intended top load with a 125 percent safety factor and shall exceed NFPA requirements of a minimum 50 mph (80 kph) wind when in a fully raised and unguyed position. The tower shall be of a compact design with a total weight of approximately 111 lbs. / 50.3 kg.  The light tower shall not exceed 150 lbs. / 68 kg.

The tower tubular sections shall be constructed of high strength, heat-treated 6061-T6 aluminum tubes and collars.  Each tube shall be protected by low friction synthetic collars for smooth operation and long life.  Bumpers shall be designed to reduce shock on extension and retraction.  All exterior surfaces shall be anodized for long life and fasteners shall be stainless steel for corrosion resistance.  

Nesting System

The tower shall have an “auto-stow” function.  A double click of the mast down button will stow, retract, and shut power off to the unit.   An integrated saddle assembly with synthetic, non-marring rests shall be provided for the tower and flood light assembly in the nested position.

Floodlight Rotation and Tilt Operation

The tower shall be equipped with a Will Burt Model RCP (remote control positioner) to control the rotation and direction of the light. The remote control positioner unit shall be equipped with two (2) gear motors; one for rotation and one for the floodlight bank.   The positioner shall also rotate the floodlight assembly from zero to 355 degrees and tilt the floodlight assembly from 0 to 337 degrees.

Choose controller option(s)
Hand-held Wired Remote Control  

A safety yellow in color for high visibility, hand held remote control pendant, connected to a quick-disconnect, 25 ft. (7.62 meter) coiled cord shall be provided to control the tower.  All functions of the tower shall be accessible through this remote control including elevating with “auto-up” ability, lowering with “auto-stow” ability, rotation and tilting of the floodlight assembly and floodlight switching.  An auxiliary power button shall also be included to control optional equipment such as strobe lights or a camera that is mounted to the mast.  An emergency stop button shall be integrated into the hand held control for added safety or shall be located on the junction box. Each button of the controller shall have a corresponding LED light that provides operational feedback.  An LED display that includes alphanumeric feedback shall be located in the center of the controller.  This display shall provide operational feedback and error codes if they occur.

Hand-held Wireless Remote Control 
 
A safety yellow in color for high visibility, wireless hand held remote control with a range of 100 feet (30.5 meters) and unique transmitting and receiving addresses to eliminate interference shall be provided to control the tower.  All functions of the tower shall be accessible through the wireless remote control including elevating with “auto-up” ability, lowering with “auto-stow” ability, rotation and tilting of the floodlight assembly and floodlight switching.  An auxiliary power button shall also be included to control optional equipment such as strobe lights or a camera that is mounted to the mast.  Each button of the controller shall have a corresponding LED light that provides operational feedback.  An LED display that includes alphanumeric feedback shall be located in the center of the controller.  This display shall provide operational feedback and error codes if they occur.

Panel-mount Control

A panel mount controller for installation on the vehicle shall be provided to control the tower.  All functions of the tower shall be accessible through the panel mount controller including elevating with “auto-up” ability, lowering with “auto-stow” ability, rotation and tilting of the floodlight assembly and floodlight switching.  An auxiliary power button shall also be included to control optional equipment such as strobe lights or a camera that is mounted to the mast.  Each button of the controller shall have a corresponding LED light that provides operational feedback.  An LED display that includes alphanumeric feedback shall be located in the center of the controller.  This display shall provide operational feedback and error codes if they occur.

Pneumatic Controls

The pneumatic controls to raise and lower the tower shall include an air regulator and solenoid valves.  Lights will be operational within approximately 8 seconds from elevation initiation.  The tower shall be able to be fully elevated in approximately 50 seconds.  In the event of malfunction of the elevating system while the tower is in operation or being deployed, a method of limiting the rate of descent shall be provided to prevent injury to personnel or damage to the equipment.
Two allen keys as well as directions are included under the cover to fold the mast into the saddle if manual stowage of mast is required.  
The air supply for pneumatic operation of the tower shall be from an integral compressor with air regulator.  

Electrical Installation

The wiring harness for the floodlights, accessories, and remote control positioner shall be internally routed through telescoping aluminum tubing with a highly flexible coil cord.  

Installer supplied 12 or 24 volt electrical wiring shall be provided with electrical connections at the tower assembly in conjunction with appropriate electrical power for the floodlights.  The installer as required by manufacturer’s installation guidelines shall provide appropriate wiring from the circuit breaker panel for connection to the tower.   The electric power to the tower and light units shall automatically disconnect whenever the tower is in the nested position.   

The tower operation area shall be illuminated automatically by a look up light whenever the tower is in operation.  Any upward movement of the tower from the nested position shall energize a red warning light in the cab and a secondary light located at the tower control area.  In addition, the installer shall provide parking brake interlocks and other equipment as required by applicable NFPA standards. 

Floodlight System

Two (2) Fire Research Optimum model OPA100-M15 lamphead shall be provided.  The lamphead shall have one (1) quartz halogen 1500 watt 240 volt bulb. Each bulb will draw 6.25 amps and generate 35,000 lumens for a total of 70,000 lumens. The bulb shall be accessible through the front. The lamphead shall incorporate a vacuum deposit polished reflector to produce a uniform beam that lights up an area 100° vertically by 150° horizontally. The lamphead shall have a heat dissipating curved front lens. The curve of the lens shall have a radius of 5.16 inches to optimize light emission. The lamphead shall be no more than 4 3/4" deep by 5 1/8" high by 14 1/8" wide. Lamphead and brackets shall be powder coated white.

Warranty

The tower assembly shall carry a two (2) year parts and labor warranty.   Exact provisions of such warranty shall be provided with the proposal and at time of delivery of product.

Labeling and NFPA Compliance

Essential operating instructions and warning labels shall be provided in compliance to applicable OSHA, SAE, and NFPA standards.  Appropriate labels on the "hazards of electrocution" associated with the operation of a light tower shall be installed in the appropriate areas.

A label shall be provided at the operator’s position by the installer with the following information:
1.  Extended height of the tower from the ground.
2.  Bulb replacement data.

The tower and installation shall be in full compliance to applicable sections of the current NFPA 1901 Standard.

Testing and Quality Assurance

The tower manufacturer shall be ISO 9001:2008 certified. In addition, quality control and manufacturer testing shall be completed prior to shipment of the tower.   The final installer shall test the operation of the tower for a minimum of 2 hours at full load, with testing documentation provided upon delivery.

Manuals

Detailed service, parts, operating, and installation manuals shall be provided by the tower manufacturer.   Samples of such manuals shall be provided on request.  A CD ROM manual will be provided to the end user.