WILL-BURT LIGHT TOWER SPECIFICATIONS
NS 1.5-150-2 Whelen Pioneer Flood 12 VDC
Model Number 720511840

A Will-Burt Night Scan light tower shall be provided.   The horizontal surface mounted tower shall be raised electrically.

Mounting provisions shall be provided with the assembly.   The installation of unit shall be as follows:
1.  Light tower installation location: 
2.  Floodlight and tower control location:

Design and Construction

The tower shall be constructed of an extruded aluminum tube.  The tower shall have an extended height of approximately 5 ft. / 1.5 m above the mounting location and a stowed height of approximately 10.375" / 26.4 cm above the mounting surface.  The tower shall be approximately 28.625” / 72.7 cm wide by 73.875” / 187.6 cm in length.  The tower shall be designed to sustain the intended top load with a 125 percent safety factor and shall exceed NFPA requirements of a minimum 50 mph (80 kph) wind when in a fully raised and unguyed position. The tower shall be of a compact design with a total weight of approximately 78 lbs. / 35.4 kg.  The light tower shall not exceed 100 lbs. / 46 kg.

The tower tubular section shall be constructed of high strength, heat-treated 6061-T6 aluminum tube.  Bumpers shall be designed to reduce shock on extension and retraction.  All exterior surfaces shall be anodized for long life and fasteners shall be stainless steel for corrosion resistance.  

Floodlight Rotation and Tilt Operation

The tower shall be equipped with a Will Burt Model RCP (remote control positioner) to control the rotation and direction of the light. The remote control positioner unit shall be equipped with two (2) gear motors; one for rotation and one for tilting the floodlight bank.   

Hand-held Wired Remote Control  

A hand held remote control pendant, connected to a 20 ft. (6 meter) cord shall be provided to control the tower.  All functions of the tower shall be accessible through this remote control including elevating and lowering, rotation and tilting of the floodlight assembly and floodlight switching.  

Electrical Installation

The wiring harness for the floodlights, accessories, and remote control positioner shall be internally routed through the aluminum tubing.  

Installer supplied 12 or 24 volt electrical wiring shall be provided with electrical connections at the tower assembly in conjunction with appropriate electrical power for the floodlights.  The installer as required by manufacturer’s installation guidelines shall provide appropriate wiring from the circuit breaker panel for connection to the tower.   
The installer shall provide parking brake interlocks and other equipment as required by applicable NFPA standards. 

Floodlight System

Two (2) Whelen Pioneer Plus™ Model # PFP1 shall be provided. The 75 watt +12v DC Pioneer lighthead shall incorporate Super-LED® single flood light installed in a die-cast white powder coated aluminum housing. The PFP1 configuration shall consist of 30 white Super-LEDs, a clear optic collimator/metalized reflector assembly and a clear non-optic polycarbonate lens. Each Pioneer flood light shall have 8,000 usable lumens for a total of 16,000 lumens.  The lens/reflector assembly shall utilize a liquid injected molded silicone gasket to be resistant to water, moisture, dust, and other environmental conditions. The hard coated lens shall provide extended life/luster protection against UV and chemical stresses. The PFP1 shall be shall be vibration resistant. The Pioneer™ PC boards shall be conformal coated for additional protection. Two breathable membrane patches shall be installed to the bottom of the housing to maintain a consistent internal pressure. The PFP1 shall have extended LED operation with low current consumption and low operating temperature.  The fixture shall measure H=4.125”, W=8.125”, D=2.50”

Warranty

The tower assembly shall carry a two (2) year parts and labor warranty.   Exact provisions of such warranty shall be provided with the proposal and at time of delivery of product.

Labeling and NFPA Compliance

Essential operating instructions and warning labels shall be provided.  Appropriate labels on the "hazards of electrocution" associated with the operation of a light tower shall be installed in the appropriate areas.

A label shall be provided at the operator’s position by the installer with the following information:
1.  Extended height of the tower from the ground.
2.  Bulb replacement data.

Testing and Quality Assurance

The tower manufacturer shall be ISO 9001:2008 certified. In addition, quality control and manufacturer testing shall be completed prior to shipment of the tower.   The final installer shall test the operation of the tower for a minimum of 2 hours at full load, with testing documentation provided upon delivery.

Manuals

Detailed service, parts, operating, and installation manuals shall be provided by the tower manufacturer.   Samples of such manuals shall be provided on request.  A CD ROM manual will be provided to the end user.